**C6 Inside Rear View Mirror Vibration**

Finally figured out how to fix my C6 rear view mirror vibration – about a 15-minute fix – Tom G.:

1. Remove mirror by twisting at base of mirror counter-clockwise about ¼ turn.
2. Unplug wire harness connector (press locking tab slightly and pull)
3. Remove 3 t-8 torx head screws
4. Remove 3 small pins (they are probably slightly bent)
5. Cut 3 5/64 “drill bits to the length of the removed pins using the solid part of the bits
6. Insert new pins in mirror
7. Install 3 t-8 screws and tighten
8. Reinsert wiring harness
9. Attach mirror with ¼ turn clockwise motion – notice that there is no more vibration.

Below is photo of the removed mirror with view of t8 screws and new pins installed